/* USER CODE BEGIN Header */
/**
  ******************************************************************************
  * @file    stm32f0xx_hal_conf.h
  * @brief   HAL configuration file.
  ******************************************************************************
  * @attention
  *
  * Copyright (c) 2016 STMicroelectronics.
  * All rights reserved.
  *
  * This software is licensed under terms that can be found in the LICENSE file
  * in the root directory of this software component.
  * If no LICENSE file comes with this software, it is provided AS-IS.
  *
  ******************************************************************************
  */
/* USER CODE END Header */

/* Define to prevent recursive inclusion -------------------------------------*/
#ifndef __STM32F0xx_HAL_CONF_H
#define __STM32F0xx_HAL_CONF_H

#ifdef __cplusplus
 extern "C" {
#endif

/* Exported types ------------------------------------------------------------*/
/* Exported constants --------------------------------------------------------*/

/* ########################## Module Selection ############################## */
/**
  * @brief This is the list of modules to be used in the HAL driver
  */
#define HAL_MODULE_ENABLED
  /*#define HAL_ADC_MODULE_ENABLED   */
/*#define HAL_CRYP_MODULE_ENABLED   */
/*#define HAL_CAN_MODULE_ENABLED   */
/*#define HAL_CEC_MODULE_ENABLED   */
/*#define HAL_COMP_MODULE_ENABLED   */
/*#define HAL_CRC_MODULE_ENABLED   */
/*#define HAL_CRYP_MODULE_ENABLED   */
/*#define HAL_TSC_MODULE_ENABLED   */
/*#define HAL_DAC_MODULE_ENABLED   */
/*#define HAL_I2S_MODULE_ENABLED   */
/*#define HAL_IWDG_MODULE_ENABLED   */
/*#define HAL_LCD_MODULE_ENABLED   */
/*#define HAL_LPTIM_MODULE_ENABLED   */
/*#define HAL_RNG_MODULE_ENABLED   */
/*#define HAL_RTC_MODULE_ENABLED   */
#define HAL_SPI_MODULE_ENABLED
/*#define HAL_TIM_MODULE_ENABLED   */
/*#define HAL_UART_MODULE_ENABLED   */
/*#define HAL_USART_MODULE_ENABLED   */
/*#define HAL_IRDA_MODULE_ENABLED   */
/*#define HAL_SMARTCARD_MODULE_ENABLED   */
/*#define HAL_SMBUS_MODULE_ENABLED   */
/*#define HAL_WWDG_MODULE_ENABLED   */
/*#define HAL_PCD_MODULE_ENABLED   */
#define HAL_CORTEX_MODULE_ENABLED
#define HAL_DMA_MODULE_ENABLED
#define HAL_FLASH_MODULE_ENABLED
#define HAL_GPIO_MODULE_ENABLED
#define HAL_EXTI_MODULE_ENABLED
#define HAL_PWR_MODULE_ENABLED
#define HAL_RCC_MODULE_ENABLED
#define HAL_I2C_MODULE_ENABLED

/* ########################## HSE/HSI Values adaptation ##################### */
/**
  * @brief Adjust the value of External High Speed oscillator (HSE) used in your application.
  *        This value is used by the RCC HAL module to compute the system frequency
  *        (when HSE is used as system clock source, directly or through the PLL).
  */
#if !defined  (HSE_VALUE)
  #define HSE_VALUE    ((uint32_t)8000000) /*!< Value of the External oscillator in Hz */
#endif /* HSE_VALUE */

/**
  * @brief In the following line adjust the External High Speed oscillator (HSE) Startup
  *        Timeout value
  */
#if !defined  (HSE_STARTUP_TIMEOUT)
  #define HSE_STARTUP_TIMEOUT    ((uint32_t)100)   /*!< Time out for HSE start up, in ms */
#endif /* HSE_STARTUP_TIMEOUT */

/**
  * @brief Internal High Speed oscillator (HSI) value.
  *        This value is used by the RCC HAL module to compute the system frequency
  *        (when HSI is used as system clock source, directly or through the PLL).
  */
#if !defined  (HSI_VALUE)
  #define HSI_VALUE    ((uint32_t)8000000) /*!< Value of the Internal oscillator in Hz*/
#endif /* HSI_VALUE */

/**
  * @brief In the following line adjust the Internal High Speed oscillator (HSI) Startup
  *        Timeout value
  */
#if !defined  (HSI_STARTUP_TIMEOUT)
 #define HSI_STARTUP_TIMEOUT   ((uint32_t)5000) /*!< Time out for HSI start up */
#endif /* HSI_STARTUP_TIMEOUT */

/**
  * @brief Internal High Speed oscillator for ADC (HSI14) value.
  */
#if !defined  (HSI14_VALUE)
#define HSI14_VALUE ((uint32_t)14000000) /*!< Value of the Internal High Speed oscillator for ADC in Hz.
                                             The real value may vary depending on the variations
                                             in voltage and temperature.  */
#endif /* HSI14_VALUE */

/**
  * @brief Internal High Speed oscillator for USB (HSI48) value.
  */
#if !defined  (HSI48_VALUE)
  #define HSI48_VALUE ((uint32_t)48000000) /*!< Value of the Internal High Speed oscillator for USB in Hz.
                                             The real value may vary depending on the variations
                                             in voltage and temperature.  */
#endif /* HSI48_VALUE */

/**
  * @brief Internal Low Speed oscillator (LSI) value.
  */
#if !defined  (LSI_VALUE)
  #define LSI_VALUE  ((uint32_t)40000)
#endif /* LSI_VALUE */                      /*!< Value of the Internal Low Speed oscillator in Hz
                                             The real value may vary depending on the variations
                                             in voltage and temperature.  */
/**
  * @brief External Low Speed oscillator (LSI) value.
  */
#if !defined  (LSE_VALUE)
  #define LSE_VALUE  ((uint32_t)32768)    /*!< Value of the External Low Speed oscillator in Hz */
#endif /* LSE_VALUE */

/**
  * @brief Time out for LSE start up value in ms.
  */
#if !defined  (LSE_STARTUP_TIMEOUT)
  #define LSE_STARTUP_TIMEOUT    ((uint32_t)5000)   /*!< Time out for LSE start up, in ms */
#endif /* LSE_STARTUP_TIMEOUT */

/* Tip: To avoid modifying this file each time you need to use different HSE,
   ===  you can define the HSE value in your toolchain compiler preprocessor. */

/* ########################### System Configuration ######################### */
/**
  * @brief This is the HAL system configuration section
  */
#define  VDD_VALUE                    ((uint32_t)3300) /*!< Value of VDD in mv */
#define  TICK_INT_PRIORITY            ((uint32_t)3)    /*!< tick interrupt priority (lowest by default)  */
                                                                              /*  Warning: Must be set to higher priority for HAL_Delay()  */
                                                                              /*  and HAL_GetTick() usage under interrupt context          */
#define  USE_RTOS                     0
#define  PREFETCH_ENABLE              1
#define  INSTRUCTION_CACHE_ENABLE     0
#define  DATA_CACHE_ENABLE            0
#define  USE_SPI_CRC                     0U

#define  USE_HAL_ADC_REGISTER_CALLBACKS         0U /* ADC register callback disabled       */
#define  USE_HAL_CAN_REGISTER_CALLBACKS         0U /* CAN register callback disabled       */
#define  USE_HAL_COMP_REGISTER_CALLBACKS        0U /* COMP register callback disabled      */
#define  USE_HAL_CEC_REGISTER_CALLBACKS         0U /* CEC register callback disabled       */
#define  USE_HAL_DAC_REGISTER_CALLBACKS         0U /* DAC register callback disabled       */
#define  USE_HAL_I2C_REGISTER_CALLBACKS         0U /* I2C register callback disabled       */
#define  USE_HAL_SMBUS_REGISTER_CALLBACKS       0U /* SMBUS register callback disabled     */
#define  USE_HAL_UART_REGISTER_CALLBACKS        0U /* UART register callback disabled      */
#define  USE_HAL_USART_REGISTER_CALLBACKS       0U /* USART register callback disabled     */
#define  USE_HAL_IRDA_REGISTER_CALLBACKS        0U /* IRDA register callback disabled      */
#define  USE_HAL_SMARTCARD_REGISTER_CALLBACKS   0U /* SMARTCARD register callback disabled */
#define  USE_HAL_WWDG_REGISTER_CALLBACKS        0U /* WWDG register callback disabled      */
#define  USE_HAL_RTC_REGISTER_CALLBACKS         0U /* RTC register callback disabled       */
#define  USE_HAL_SPI_REGISTER_CALLBACKS         0U /* SPI register callback disabled       */
#define  USE_HAL_I2S_REGISTER_CALLBACKS         0U /* I2S register callback disabled       */
#define  USE_HAL_TIM_REGISTER_CALLBACKS         0U /* TIM register callback disabled       */
#define  USE_HAL_TSC_REGISTER_CALLBACKS         0U /* TSC register callback disabled       */
#define  USE_HAL_PCD_REGISTER_CALLBACKS         0U /* PCD register callback disabled       */

/* ########################## Assert Selection ############################## */
/**
  * @brief Uncomment the line below to expanse the "assert_param" macro in the
  *        HAL drivers code
  */
/* #define USE_FULL_ASSERT   1U */

/* Includes ------------------------------------------------------------------*/
/**
  * @brief Include module's header file
  */

#ifdef HAL_RCC_MODULE_ENABLED
 #include "stm32f0xx_hal_rcc.h"
#endif /* HAL_RCC_MODULE_ENABLED */

#ifdef HAL_GPIO_MODULE_ENABLED
 #include "stm32f0xx_hal_gpio.h"
#endif /* HAL_GPIO_MODULE_ENABLED */

#ifdef HAL_EXTI_MODULE_ENABLED
  #include "stm32f0xx_hal_exti.h"
#endif /* HAL_EXTI_MODULE_ENABLED */

#ifdef HAL_DMA_MODULE_ENABLED
  #include "stm32f0xx_hal_dma.h"
#endif /* HAL_DMA_MODULE_ENABLED */

#ifdef HAL_CORTEX_MODULE_ENABLED
 #include "stm32f0xx_hal_cortex.h"
#endif /* HAL_CORTEX_MODULE_ENABLED */

#ifdef HAL_ADC_MODULE_ENABLED
 #include "stm32f0xx_hal_adc.h"
#endif /* HAL_ADC_MODULE_ENABLED */

#ifdef HAL_CAN_MODULE_ENABLED
 #include "stm32f0xx_hal_can.h"
#endif /* HAL_CAN_MODULE_ENABLED */

#ifdef HAL_CEC_MODULE_ENABLED
 #include "stm32f0xx_hal_cec.h"
#endif /* HAL_CEC_MODULE_ENABLED */

#ifdef HAL_COMP_MODULE_ENABLED
 #include "stm32f0xx_hal_comp.h"
#endif /* HAL_COMP_MODULE_ENABLED */

#ifdef HAL_CRC_MODULE_ENABLED
 #include "stm32f0xx_hal_crc.h"
#endif /* HAL_CRC_MODULE_ENABLED */

#ifdef HAL_DAC_MODULE_ENABLED
 #include "stm32f0xx_hal_dac.h"
#endif /* HAL_DAC_MODULE_ENABLED */

#ifdef HAL_FLASH_MODULE_ENABLED
 #include "stm32f0xx_hal_flash.h"
#endif /* HAL_FLASH_MODULE_ENABLED */

#ifdef HAL_I2C_MODULE_ENABLED
 #include "stm32f0xx_hal_i2c.h"
#endif /* HAL_I2C_MODULE_ENABLED */

#ifdef HAL_I2S_MODULE_ENABLED
 #include "stm32f0xx_hal_i2s.h"
#endif /* HAL_I2S_MODULE_ENABLED */

#ifdef HAL_IRDA_MODULE_ENABLED
 #include "stm32f0xx_hal_irda.h"
#endif /* HAL_IRDA_MODULE_ENABLED */

#ifdef HAL_IWDG_MODULE_ENABLED
 #include "stm32f0xx_hal_iwdg.h"
#endif /* HAL_IWDG_MODULE_ENABLED */

#ifdef HAL_PCD_MODULE_ENABLED
 #include "stm32f0xx_hal_pcd.h"
#endif /* HAL_PCD_MODULE_ENABLED */

#ifdef HAL_PWR_MODULE_ENABLED
 #include "stm32f0xx_hal_pwr.h"
#endif /* HAL_PWR_MODULE_ENABLED */

#ifdef HAL_RTC_MODULE_ENABLED
 #include "stm32f0xx_hal_rtc.h"
#endif /* HAL_RTC_MODULE_ENABLED */

#ifdef HAL_SMARTCARD_MODULE_ENABLED
 #include "stm32f0xx_hal_smartcard.h"
#endif /* HAL_SMARTCARD_MODULE_ENABLED */

#ifdef HAL_SMBUS_MODULE_ENABLED
 #include "stm32f0xx_hal_smbus.h"
#endif /* HAL_SMBUS_MODULE_ENABLED */

#ifdef HAL_SPI_MODULE_ENABLED
 #include "stm32f0xx_hal_spi.h"
#endif /* HAL_SPI_MODULE_ENABLED */

#ifdef HAL_TIM_MODULE_ENABLED
 #include "stm32f0xx_hal_tim.h"
#endif /* HAL_TIM_MODULE_ENABLED */

#ifdef HAL_TSC_MODULE_ENABLED
 #include "stm32f0xx_hal_tsc.h"
#endif /* HAL_TSC_MODULE_ENABLED */

#ifdef HAL_UART_MODULE_ENABLED
 #include "stm32f0xx_hal_uart.h"
#endif /* HAL_UART_MODULE_ENABLED */

#ifdef HAL_USART_MODULE_ENABLED
 #include "stm32f0xx_hal_usart.h"
#endif /* HAL_USART_MODULE_ENABLED */

#ifdef HAL_WWDG_MODULE_ENABLED
 #include "stm32f0xx_hal_wwdg.h"
#endif /* HAL_WWDG_MODULE_ENABLED */

/* Exported macro ------------------------------------------------------------*/
#ifdef  USE_FULL_ASSERT
/**
  * @brief  The assert_param macro is used for function's parameters check.
  * @param  expr If expr is false, it calls assert_failed function
  *         which reports the name of the source file and the source
  *         line number of the call that failed.
  *         If expr is true, it returns no value.
  * @retval None
  */
  #define assert_param(expr) ((expr) ? (void)0U : assert_failed((uint8_t *)__FILE__, __LINE__))
/* Exported functions ------------------------------------------------------- */
  void assert_failed(uint8_t* file, uint32_t line);
#else
  #define assert_param(expr) ((void)0U)
#endif /* USE_FULL_ASSERT */

#ifdef __cplusplus
}
#endif

#endif /* __STM32F0xx_HAL_CONF_H */

